Highlights:

* A heavy-duty, electric vehicle designed specifically for use in kiwifruit orchards is presented.
* We rule out the use of GPS, Time of Flight, and consumer stereo cameras as sensors suitable for autonomous navigation in this environment.
* Camera data processed using neural networks prove useful for identifying traversable space in complex scenes.
* Using a lidar and encoder information, our vehicle reliably navigates two test orchards.